BULL SAS
OpenManage Server Administrator Managed Node 

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Version:        6.5.0
Release Date:   3/28/2011

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Description

The Managed Node Service Pack provides a convenient method for updating from Dell OpenManage v6.4.0 and above. It includes the same fixes, updates, and enhancements available in the individual 6.5.0 downloads, but in a streamlined, downloadable collection that follows the industry-standard Windows® model. 

Fixes and Enhancements

- Server Administrator shows whether a Converged Network Adapter (CNA) has Fibre Channel over Ethernet (FCoE) /iSCSI over Ethernet (iSoE) capability or not. Also, Server Administrator supports new team types for CNA cards.
- A new memory redundancy mode called Double Device Data Correction (DDDC) is added.
- Support for display of Lifecycle Controller (LCC)/Unified Server Configurator (USC) version information. For this information to appear, the minimum iDRAC version on monolithic systems is 1.70 and on modular systems is 3.20. If  iDRAC is installed, Server Adminsitrator displays the version of LCC. If BMC is instaled, Server Admisntrator displays the version of USC.
- Support for 32x32 GB DIMM for Server Administrator to show the correct memory capacity.

Added support for the following operating systems:
	- VMware ESX 4.0 U3
	- VMware ESX 4.1 U1
	- VMware ESXi 4.1 U1
	- VMware ESXi 4.0 U3
	- Citrix Xen Server 5.6 FP1
	- Windows Small Business Server 2011

Deprecated the following operating systems:
	- Red Hat Enterprise Linux 4.x
	- VMware ESX 4.0 U2 
	- VMware ESX 4.1 
	- VMware ESXi 4.0 U2 
	- VMware ESXi 4.1 
	- Citrix Xen Server 5.6 

Compatibility
Systems				Operating Systems
NovaScale R410 F2			Microsoft Windows Server 2008 R2
NovaScale R430 F2			Microsoft Windows Server 2008 x64
NovaScale R440 F2			Microsoft Windows Server 2008 x86
NovaScale R450 F2			Microsoft Windows Server 2003 x64
NovaScale R460 F2			Microsoft Windows Server 2003 x86
NovaScale R480 F2			
NovaScale T810 F2			
NovaScale T820 F2	
NovaScale T840 F2  
NovaScale T860 F2
Installation Instructions
Installation
1.Double click on the MSP file or enter the following in a command-prompt window:
	Msiexec.exe /p OM-SrvAdmin-SP-WIN-6.5.0-2247_A01.12.msp