BULL SAS
OpenManage Server Administrator Managed Node 

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Version:        6.5.0
Release Date:   3/28/2011

~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Description

OpenManage Server Administrator Managed Node provides easy-to-use management and administration of local and remote systems through a comprehensive set of integrated management services. Server Administrator resides solely on the system being managed and is accessible both locally and remotely from the Server Administrator home page. 

Fixes and Enhancements

- Server Administrator shows whether a Converged Network Adapter (CNA) has Fibre Channel over Ethernet (FCoE) /iSCSI over Ethernet (iSoE) capability or not. Also, Server Administrator supports new team types for CNA cards.
- A new memory redundancy mode called Double Device Data Correction (DDDC) is added.
- Support for display of Lifecycle Controller (LCC)/Unified Server Configurator (USC) version information. For this information to appear, the minimum iDRAC version on monolithic systems is 1.70 and on modular systems is 3.20. If  iDRAC is installed, Server Adminsitrator displays the version of LCC. If BMC is instaled, Server Admisntrator displays the version of USC.
- Support for 32x32 GB DIMM for Server Administrator to show the correct memory capacity.

Added support for the following operating systems:
	- VMware ESX 4.0 U3
	- VMware ESX 4.1 U1
	- VMware ESXi 4.1 U1
	- VMware ESXi 4.0 U3
	- Citrix Xen Server 5.6 FP1
	- Windows Small Business Server 2011

Deprecated the following operating systems:
	- Red Hat Enterprise Linux 4.x
	- VMware ESX 4.0 U2 
	- VMware ESX 4.1 
	- VMware ESXi 4.0 U2 
	- VMware ESXi 4.1 
	- Citrix Xen Server 5.6 

Compatibility
Systems				Operating Systems
NovaScale R410 F2			Microsoft Windows Server 2008 R2
NovaScale R430 F2			Microsoft Windows Server 2008 x64
NovaScale R440 F2			Microsoft Windows Server 2008 x86
NovaScale R450 F2			Microsoft Windows Server 2003 x64
NovaScale R460 F2			Microsoft Windows Server 2003 x86
NovaScale R480 F2			
NovaScale T810 F2			
NovaScale T820 F2	
NovaScale T840 F2  
NovaScale T860 F2
Installation Instructions
Extract Files
1.Browse to the location where you downloaded the file and double-click to unzip the download package.
2.Specify the location to unzip the files (default is "C:\OpenManage").
3.Click on the Unzip button to extract the files.

Installation
1.Browse to the location where the files were unzipped.
2.Double-click the setup.exe file under the "windows" subdirectory and follow the on-screen instructions.

Note: Consult the OpenManage Server Administrator Installation Guide under the "docs" subfolder in the extracted location for detailed installation instructions.